2.5. Histogram dialog
| 2. Image Structure Related Dialogs |

### 2.5. Histogram dialog

Figure 14.16. The Histogram dialog

The Histogram dialog shows you information about the statistical distribution of color values in the active layer or selection. This information is often useful when you are trying to color balance an image. However, the Histogram dialog is purely informational: nothing you do with it will cause any change to the image. If you want to perform a histogram-based color correction, use the Levels tool.

#### 2.5.1. Activating the dialog

The “Histogram” dialog is a dockable dialog; see the section Section 2.3, “Dialogs and Docking” for help on manipulating it.

You can access it:

- from the image menu: Windows → Dockable Dialogs → Histogram.

- from the Tab menu in any dockable dialog by clicking on and selecting Add Tab → Histogram,

- from the image menu: Colors → Info → Histogram.

In the Windows menu, there is a list of detached windows which exists only if at least one dialog remains open. In this case, you can raise the “Histogram” dialog from the image-menu: Windows → Histogram.

#### 2.5.2. About Histograms

In GIMP, each layer of an image can be decomposed into one or more color channels: for an RGB image, into R, G, and B channels; for a grayscale image, into a single Value channel. Layers that support transparency have an additional channel, the alpha channel. Each channel supports a range of intensity levels from 0 to 255 (integer valued). Thus, a black pixel is encoded by 0 on all color channels; a white pixel by 255 on all color channels. A transparent pixel is encoded by 0 on the alpha channel; an opaque pixel by 255.

For RGB images, it is convenient to define a Value “pseudochannel ”. This is not a real color channel: it does not reflect any information stored directly in the image. Instead, the Value at a pixel is given by the equation `V = max(R,G,B)`. Essentially, the Value is what you would get at that pixel if you converted the image to Grayscale mode.

For more information on channels, please consult the Section 1, “ Image Types ”.

#### 2.5.3. Using the Histogram dialog

The active layer name is shown at the top of the dialog.

Channel

  Figure 14.17. Channel options for an RGB layer with alpha channel

  This allows you to select which channel to use. The possibilities depend on the layer type of the active layer. Here are the entries you might see, and what they mean:

  Value

    For RGB and Grayscale images, this shows the distribution of brightness values across the layer. For a grayscale image, these are read directly from the image data. For an RGB image, they are taken from the Value pseudochannel.

    For an indexed image, the “Value” channel actually shows the distribution of frequencies for each colormap index: thus, it is a “pseudocolor” histogram rather than a true color histogram.

  Red, Green, Blue

    These only appear for layers from RGB images. They show the distribution of intensity levels for the Red, Green, or Blue channels respectively.

  Alpha

    This shows the distribution of opacity levels. If the layer is completely opaque or completely transparent, the histogram will consist of a single bar on the left or right edge.

  RGB

    Figure 14.18. Combined histograms of R, G, and B channels.

    This entry, only available for RGB layers, shows the R, G, and B histograms superimposed, so that you can see all of the color distribution information in a single view.

Linear/Logarithmic buttons

  Figure 14.19. The histogram shown at the top, changed to logarithmic mode.

  These buttons determine whether the histogram will be displayed using a linear or logarithmic Y axis. For images taken from photographs, the linear mode is most commonly useful. For images that contain substantial areas of constant color, though, a linear histogram will often be dominated by a single bar, and a logarithmic histogram will often be more useful.

Range Setting

  Figure 14.20. Dialog aspect after range fixing.

  You can restrict the analysis, for the statistics shown at the bottom of the dialog, to a limited range of values if you wish. You can set the range in one of three ways:

  - Click and drag the pointer across the histogram display area, from the lowest level to the highest level of the range you want.

  - Click and drag the black or white triangles on the slider below the histogram.

  - Use the spinbutton entries below the slider (left entry: bottom of range; right entry: top of range).

Statistics

  At the bottom of the dialog some basic statistics are shown describing the distribution of channel values, restricted to the selected range:

  - Mean : the mean value of the interval in the selected channel.

  - Std Dev : Standard deviation. Gives an idea about how homogeneous the distribution of values in the interval is.

  - Median : For example, the value of the fiftieth peak in a 100 peaks interval.

  - Pixels : The number of pixels in the active layer or selection.

  - Count : The number of pixels in a peak (when you click on the histogram) or in the interval.

  - Percentile : The ratio between the number of pixels in the interval and the total number of pixels in the active layer or selection.

2.4. Colormap Dialog |  | 2.6. Navigation Dialog